Instrument name here

1. Commands issued by service at initialization 


    _toDevice.write("APP\r".getBytes());


    getInstrumentAttention(3);// "ECHO OFF\r".,”\r”
2. Commands issued by service for safe mode, if applicable

N/A

3. Device metadata returned in SIAM datastream
powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.serialadc.SerialAdc$Attributes

captureParams=ALL

serviceName=Mooring power can s/n 2

parentID=1446

maxSummarySamples=0

currentLimitMa=3000

packetSetSize=10

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

defaultSkipInterval=0

statusMinSamples=10

extendedVersion=UNK

frameworkVersion=$Name: june09_2006 $

errCacheLimit=5

UUID=3e29b0a1-bdc4-11da-855d-00306e389969

powerWarningLow=9.0

powerPolicy=ALWAYS

timeSynch=false

powerOkLow=10.0

maxSampleTries=3

isiID=1547

powerStatusChannel=ADC99

peakCurrentMa=5000

summaryTriggerCount=0

dataCountCheck=true

sampleTimeoutMsec=5000

commPowerPolicy=SAMPLING

serviceStatus=2

logTimeSync=true

startDelayMsec=10000

isiID = 1547

serviceName = Mooring power can s/n 2

powerPolicy = always

commPowerPolicy = sampling

sampleSchedule = 600

captureParams = ALL

dataCountCheck = true

logTimeSync = true

powerStatusChannel = ADC99

powerWarningLow=9.0

powerOkLow=10.0

statusMinSamples = 10

currentLimitMa = 3000

sampleTimeoutMsec=15000

UUID = 3e29b0a1-bdc4-11da-855d-00306e389969

VERSION:

MOOS POWER SYSTEM DAQ 0.7

built on May  9 2006 at 21:57:13

CVS tag "$Name:  $"

CONFIGURATION:

ADC00 S00 C01 P0001000 T0000000 D0 L0 A1

ADC01 S00 C02 P0001000 T0000000 D0 L0 A1

ADC02 S00 C03 P0001000 T0000000 D0 L0 A1

ADC03 S00 C04 P0001000 T0000000 D0 L0 A1

ADC04 S00 C05 P0001000 T0000000 D0 L0 A1

ADC05 S00 C06 P0001000 T0000000 D0 L0 A1

ADC10 S01 C01 P0001000 T0000000 D0 L0 A1

ADC11 S01 C02 P0001000 T0000000 D0 L0 A1

ADC12 S01 C03 P0001000 T0000000 D0 L0 A1

ADC13 S01 C04 P0001000 T0000000 D0 L0 A1

ADC14 S01 C05 P0001000 T0000000 D0 L0 A1

ADC15 S01 C06 P0001000 T0000000 D0 L0 A1

ADC20 S02 C01 P0001000 T0000000 D0 L0 A1

ADC21 S02 C02 P0001000 T0000000 D0 L0 A1

ADC22 S02 C03 P0001000 T0000000 D0 L0 A1

ADC23 S02 C04 P0001000 T0000000 D0 L0 A1

ADC24 S02 C05 P0001000 T0000000 D0 L0 A1

ADC25 S03 C01 P0001000 T0000000 D0 L0 A1

ADC26 S03 C02 P0001000 T0000000 D0 L0 A1

ADC27 S03 C03 P0001000 T0000000 D0 L0 A1

ADC28 S03 C04 P0001000 T0000000 D0 L0 A1

ADC29 S03 C05 P0001000 T0000000 D0 L0 A1

ADC30 S04 C01 P0000250 T0000000 D0 L0 A1

ADC31 S04 C02 P0000250 T0000000 D0 L0 A1

ADC32 S04 C03 P0001000 T0000000 D1 L0 A1

ADC35 S05 C01 P0000250 T0000000 D0 L0 A1

ADC36 S05 C02 P0000250 T0000000 D0 L0 A1

ADC37 S05 C03 P0001000 T0000000 D2 L0 A1

ADC42 S06 C11 P0000250 T0000000 D0 L2 A1

ADC43 S06 C10 P0010000 T0000000 D0 L0 A1

ADC48 S06 C01 P0000250 T0000000 D0 L0 A1

DO00 S-1 C-1 E0000000 D0000000  O0 A1

DO01 S04 C05 E0000100 D0000200  O1 A1

DO02 S05 C05 E0000100 D0000200  O1 A1

DO03 S06 C00 E0000000 D0000000  O0 A1

DO04 S06 C01 E0000000 D0000000  O1 A1

DO05 S06 C02 E0000200 D0000050  O0 A1

DO06 S06 C03 E0000200 D0000050  O0 A1

GFZ00 S04 C06 A1

GFL00 S04 C06 A1

GFH00 S04 C06 A1

GFT00 S04 C06 A1

GFZ01 S08 C06 A1

GFL01 S08 C06 A1

GFH01 S08 C06 A1

GFT01 S08 C06 A1

GF P0060000 S0000950 A1

ENV P0010000 A1

WS00 S00 C07 P0010000 A1

WS01 S01 C07 P0010000 A1

CALIBRATION:

S00 C01 G-3.0520e-04 O+0.0000e+00

S00 C02 G-3.0520e-04 O+0.0000e+00

S00 C03 G+1.9940e-03 O+0.0000e+00

S00 C04 G+1.9940e-03 O+0.0000e+00

S00 C05 G+3.0520e-04 O+0.0000e+00

S00 C06 G+3.0520e-04 O+0.0000e+00

S01 C01 G-3.0520e-04 O+0.0000e+00

S01 C02 G-3.0520e-04 O+0.0000e+00

S01 C03 G+1.9940e-03 O+0.0000e+00

S01 C04 G+1.9940e-03 O+0.0000e+00

S01 C05 G+3.0520e-04 O+0.0000e+00

S01 C06 G+3.0520e-04 O+0.0000e+00

S02 C01 G+6.1030e-04 O+0.0000e+00

S02 C02 G+6.1030e-04 O+0.0000e+00

S02 C03 G+1.9940e-03 O+0.0000e+00

S02 C04 G+1.5320e-01 O-2.7315e+02

S02 C05 G+1.5320e-01 O-2.7315e+02

S03 C01 G+6.1030e-04 O+0.0000e+00

S03 C02 G+6.1030e-04 O+0.0000e+00

S03 C03 G+1.9940e-03 O+0.0000e+00

S03 C04 G+1.5320e-01 O-2.7315e+02

S03 C05 G+1.5320e-01 O-2.7315e+02

S04 C01 G+3.0520e-04 O+0.0000e+00

S04 C02 G+3.0520e-04 O+0.0000e+00

S04 C03 G+1.5300e-02 O+0.0000e+00

S05 C01 G+3.0520e-04 O+0.0000e+00

S05 C02 G+3.0520e-04 O+0.0000e+00

S05 C03 G+5.6080e-04 O+0.0000e+00

S06 C11 G+7.5720e-07 O+0.0000e+00

S06 C10 G+1.0000e+00 O-1.6384e+04

S06 C01 G+1.8300e-05 O+0.0000e+00

GF S04 C06 G+3.8150e-08 O+0.0000e+00

GF S08 C06 G+3.8150e-08 O+0.0000e+00

CALIBRATION REV "$Revision: 1.13 $"

4. Instrument-specific service properties
5. Initial service property values for this deployment
6. Results of acceptance test procedures
N/A

7. Known-service bugs/deficiencies

Issues “EXIT\r” on shutdown instrument (stops P2 app)






