As a means of providing a key to the items on the drill sled picture

The yellow items are new hardware.  Primarily brackets and mounts necessitated by the move to the Tiburon Tool Sled, and the new items to be mounted.

The pink items in the picture are purchased hardware.  These were items were required by the conversion.  The two stage high/low torque motor replaced a smaller single stage hydraulic motor.  The water pump to flush the drill bit was d

hydraulically driven on Ventana. The new one here is driven by a brushless electric motor.  A standard well drilling water swivel was added to the drill string to pass the flushing water into the drill.  On the front of the sled, the explosive cutter was not only upgraded electrically, but enlarged to allow for the increased working pressures that will be seen on Tiburon.

A pressure compensated junction box and a data concentrator pressure case were added to provide an interface with Tiburon electronics.

