DORISS/PUP Weights

(From March 4, 2004)

Weighed with an electronic scale in air and in water in the MBARI test tank

PUP (w/ cables, no VIC, no probe head) :


207 lbs.  DRY 
55 lbs.
 WET
DORISS (w/ VIC and cables and probe head):


462 lbs.  DRY 
123 lbs.  WET
Previous measurements of the probe head:


27 lbs.  DRY 

13 lbs. 
WET

DORISS/PUP together weighs 669 lbs. DRY,  178 lbs. WET with 68 lbs. deployed weight (i.e. PUP plus probe head).

The DORISS configuration no longer has the power inverter in the Electronics Housing.

The PUP configuration is two axes (Z and R) with 2 lasers, 1 light, and 1 camera; and a polypro lifting harness.

DORISS/PUP Weights

(From July, 2004)

Weighed with an electronic scale in air and in water in the MBARI test tank

PUP (w/ cables, probe head, 30 lbs ballast in back leg) :


260 lbs.  DRY

86 lbs.  WET
DORISS (w/ cables and probe head):


430 lbs.  DRY

114 lbs.  WET
VIC (by itself):


14 lbs.  DRY

7 lbs.  WET

Previous measurements of the probe head:


27 lbs.  DRY

13 lbs.  WET

DORISS/PUP together weighs 677 lbs. DRY, 194 lbs. WET with 86 lbs. deployed weight (i.e. PUP plus probe head).

The PUP configuration is three axes (Z, R, and theta) with 2 lasers, 1 light, and 1 camera; and a polypro lifting harness.

