Ventana Dive #2450
11/5/03

Deploying methane cylinder @ Invert Cliff (waypoint: Barry 1022) (using homer 36)

11:40
Launching ROV


Bounce okay

11:43
Going down (“launch time 11:40”)


Proceeding to 200 m to fill gas cylinder

11:51
@ 200 m (~9.25°C)

11:52
Started Tape 1

11:55
Cylinder acquired in manipulator and held horizontally


Flushing with seawater (10 pump strokes + 1 or 2 more)

12:02
Flushing with gas (3 times)


Cylinder moved to vertical orientation

12:04
Filled with gas


Agitating for a few minutes (“shaken not stirred”, “methane martini”)

12:08
Adding more gas


Proceeding to 400 m

12:15
@ 400 m (~7.10°C)
Adding more gas


Proceeding to 800 m

12:28
@ 800 m (~4.37°C)
Adding more gas



Can see hydrate film (nice frame grab)


Proceeding to bottom

12:35
@ 1000 m
Filling more gas

12:37
@ bottom
Looking for a flat spot to land

12:39
On bottom 1019 m


Trying to get the line in the cutter (the line is a bit long)

12:49
Last fill of cylinder

12:53
Starting Tape 2 (1:00:32? tape time)


Cutter is locked up, will try to rip with manips?

12:55
Deploying homer (#36)

12:58
Cutter is working!  Lines cut


*Pilots got a sonar grab to show location
25 m west of Invert Cliff (1019 m, 3.9°C)

Losing gas through the skinny line (check valve failed?)


Ed called from shore and suggests sticking the line into the mud


Pinched line and shoved it in the sediment (frame grab shows the burial job)

13:14
Leaving site (will do a quick tour of the cliff)

13:17
Coming up


Stopping tape (1:25:51 tape time)

