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Sheri N. White

Monterey Bay Aquarium Research Institute

7700 Sandholdt Rd.

Moss Landing, CA 95039

Phone: (831) 775-1903

Fax: (831) 775-1620

Email: sheri@mbari.org



August 28, 2002

Harris International

35 West 45th Street

New York, NY  10036

Mr. Fraser:

The 2.0 x 2.0 x 0.5 mm type 2A diamond that we ordered from you has worked out very well.  However, we feel we made need a larger diamond for this particular application –  as a calibration standard in a laser Raman spectrometer we are adapting for deep-sea use.

Could you please provide us with another quote for a type 2A diamond selected for low (group D) fluorescence with only the large parallel faces polished.  We are interested in one that is 4 x 4 mm, and 0.5 or 1.0 mm thick.  Our past diamond was square, which is fine.  Is a circular diamond (4 mm diameter) an option?  If so, please provide a quote for that as well (both 0.5 and 1.0 mm think).

You can reach me by phone or fax at the numbers above.  Thank you for your assistance.

Sincerely, 


Dr. Sheri N. White
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