IO base addresses, interrupts, jumper settings for the 

Laser Raman Single Board Computer (SBC) System

Note, most of these are the factory default settings.

The CPU board and camera do not require special settings. 

-----------------------------------------------------------------

History:

Created: 12:39 PM 5/22/01 D.Cline

Added 7404 quad serial: 1:25 PM 10/16/02 D.Cline

Revised: 2:30 PM 10/13/03 S.N.White

-----------------------------------------------------------------

               

I/O Address
Interrupt/Jumper Settings

-----------------------------------------------------------------

DMA Controller #1       0x00-0x1F     

Interrupt Controller #1 0x20-0x3F

Programmable Timer      0x40-0x5F

0

Keyboard Controller     0x60-0x6F

1

Real time clock, NMI
0x70-0x7F

8

DMA Page Registers      0x80-0x9F

Interrupt Controller #2 0xA0-0xBF

DMA Controller #2       0xC0-0xDF

Clear math coprocessor 
0xF0


   busy signal

Reset math coprocessor
0xF1

Match processor

0xF8-0xFF

13

Disable watchdog timer
0x120

Enable watchdog timer
0x121

Watchdog


0x122

Fixed disk controller
0x1F0-0x1F8

14/primary 15/secondary

Game port


0x200-0x207

Prototype card

0x300-0x31F

Reserved


0x360-0x36F

Parallel port #1

0x378-0x37F

0x3B/IRQ7

MDA video card

0x3B0-0x3BF

EGA card


0x3C0-0x3CF

CGA card


0x3D0-0x3DF

Floppy disk controller
0x3F0-0x3FF

6

Serial port #1(COM1)
0x3F8-0x3FF

4

Serial port #2(COM2)
0x2F8-0x2FF

3

7404 Quad Serial



COM3 (RS485)
0xD400
Shunt E7
10 (SW1) S1=on,S2=off,S3-4=on 


COM4 (RS232)
0xD800
Shunt E6
10 (SW2) S1-4=off 


COM5 (RS422)
0xDC00
Shunt E3
10 (SW3) S1=on,S2=off,S3-4=on 


COM6 (RS422)
0xE000
Shunt E1
10 (SW4) S1=on,S2=off,S3-4=on 

USB






11

PS/2 Mouse





12

PCI backplane card
JP1=open; JP2=2-3; JP3=all open; 





JP4= 1-2,3-4,5-6,7-8,9-10

PCI SBC card
JP1=1-2,3-4; JP3=open; JP4=1-2; JP5=1-2; 




JP6=3-5,4-6; JP7=3-5,4-6; JP8=1-2; 




JP9=1-2; JP10=1-2

interrupts 5,9,10 reserved


------------------------------------------------------------

Card Info: see vendor.txt for details

------------------------------------------------------------

