Home repeatability

1) Home Actuator

2) Measure housing to Ram thread base distance in mm

3) Extend and retract actuator 10240 counts

4) Repeat set 3 seven times

5) Extend actuator 10240 counts

6) Home Actuator

7) Measure housing to Ram thread base distance in mm

8) Repeat 2-7 two more times

Extension distance

9) Move actuator to absolute position 81920

10) Measure housing to Ram thread base distance in mm

Resolution and repeatability accuracy

11) Move actuator to absolute position 40960

12) Measure housing to Ram thread base distance in mm

13) Move actuator 40 counts out

14) Measure housing to Ram thread base distance in mm

15) Move actuator 40 counts in

16) Measure housing to Ram thread base distance in mm

17) Repeat step 13 – 16 two more times

Absolute accuracy

18) Move actuator to absolute 0

19) Measure housing to Ram thread base distance in mm

20) Move actuator to 40960

21) Measure housing to Ram thread base distance in mm

22) Repeat 18 – 21 two more times.
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