April3, 2007- note on the power board

The power board has 3 75W vicors, assuming that we are only using 30% of the power output (75W) and at that level the vicor is only 50% efficient, the overall heat dissipated would be 38W.

