My DUSBL will be ready some time in September and you can use that one.  It is a shame we didn't do yours at the same time.  I would guess it will be into November to get another one complete, but will need to check with lead time on ceramics and potting.   Potted in head, no additional boards. We connect to a serial port on MB.
NBOSI CTD, O2, OBS Chl, (no PAR), 2 ADCPs, Long Range ACOMMs, plus the new Sparton compass

capture drive is $53K with parts, labor and overhead.
I'll do an official quote when you need it, just let me know.
NBOSI, O2, Li-COR quantum sensor (Li-192SA), 2 ADCPs, ACOMMS with transducer and hydrophone array and I ordered two separate compasses but would like to use the Sparton AHRS-M2, preferably it wouldn't be inside the ADCP housing.  The other one is PNI TCM-XB which was on your call sheet but not one that was compared.

508-274-6367 cell Amy
"Jason Kapit" <jkapit@whoi.ed
DMON2

https://www.dropbox.com/s/j5yipo0cez7bze9/208016-ASM%20DMON2%20Mainboard%20and%20Flash%20Expansion%20Board.stp?dl=0
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The electronics stack weighs 1.8oz. If we add a Li-Ion battery as we often do in the Slocum gliders the weight would be 8.2 oz for the electronics and battery combined.
 
See the attached 212006-ASM print for the dimension of the DMON2 Hydrophone head. Weight in air is 5.4oz.
 
I would also be interested to know what specific features are needed from the Benthos kit.

