Dimensions:
	Max outer diameter
	85 cm

	Min outer diameter
	42 cm

	Max instrument length
	89 cm

	Approximate weight in air
	25 kg

	Approximate weight in seawater
	15 kg
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Figure 1: View of the front of EyeRIS with the illumination expanded to its max size. The diameter of the array is 85 cm.
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Figure 2: View of the front of EyeRIS with the illumination folded to its minimum size. The diameter of the array is 42 cm.
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Figure 3: View of the side of EyeRIS showing the far (92.55 cm), middle (82.44 cm), and near (72.15 cm) distances from the viewport to the imaged volume. Accounting for space for cables and connectors, the instrument length is less than 89 cm.
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