Note: 
1) File names are

 MLXXYY

ML = MARS Lab

XX = OTDR inject sea cable fiber number per ODI Connector number on fiberEndtoEndMapRevE.xls

YY = loop back fiber per  ODI Connector number on fiberEndtoEndMapRevE.xls

2) Ken used an optical power meter on ML end of loopback fiber to ensure proper connectivity.

