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Funtion

The DcsServer is generally responsible for all network management tasks, as well as most of the common internet server tasks. 

It has the following roles: 

It runs the DcsSoftware
DnsServer running DnsMasq  open source - Dnsmasq is a lightweight, easy to configure DNS forwarder and DHCP server
Nagios  -  open source  - a powerful if somewhat complicated network monitoring tool. Runs as its own webserver at http://marsdcs.shore.mbari.org/nagios/
MRTG  - open source  - Multi Router Traffic Grapher, a set of Perl scripts which generate graphs of router traffic. Actually, technically it will plot any number which can be retrieved by SNMP, but network traffic is what it was originally designed for.
Rancid   Really Awesome New Cisco confIg Differ. It's a software package which can log into a variety of network equipment (Cisco routers, switches and firewalls in this case), extract their config files, and store those config files in a version control system (CVS).
SyslogServer - MARS infrastructure syslog. Syslog is a standard UNIX protocol which allows a client to send text messages to a designated server. These messages are then timestamped and logged to disk.
SailTerminal 
Best Info Sources:

http://134.89.42.15/marswiki//DcsServer
Hardware:
HP-Proliant CPU 
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Linux – Red Hat Enterprise
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