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Function

The Secure Console Monitor (SCM) is a multi-port serial interface box. It's basically a box with 16 serial ports and an ethernet jack which allows connections from serial-to-serial and serial-to-ethernet. In the Mars system its used primarily as a serial-to-ethernet converter providing a networked, shared, convenient method for accessing the various serial consoles and backdoors scattered throughout the Mars network hardware. 

Best Information Source:

http://134.89.42.15/marswiki/SecureConsoleMonitor

Hardware:
COTS Hardware

Western Telematic SCM-16
OS: 
Software and Interfaces
DEVELOPED BY:

SOURCE CODE STATUS:
USE DOCUMENTATION:

http://134.89.42.15/marswiki/SecureConsoleMonitor?action=AttachFile&do=get&target=SecureConsoleMonitor_ManualRevD.pdf 
API DOCUMENTATION:
BUILD DOCUMENTATION:
DESIGN/CODE  DOCUMENTATION:
POSSIBLE NEXT STEPS:
None
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