Capturing Video On Ephyra


Before loading Adobe Premiere 6.5 the Sony BetaCam Deck should be turned on.  Once the BetaCam Deck is turned on a cassette could be loaded.  Rewind the cassette to the beginning.  Once the BetaCam has been turned on Adobe Premiere 6.5 can be loaded.
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Under the Start Menu select Programs -> Adobe -> Premiere 6.5 -> Premiere 6.5.  This will start up Adobe Premiere.  Upon loading user should see the Load Project Settings window.  From the Load Project Settings window highlight AVED Project TARGA 3000 NTSC R… and select OK.  This brings you into Adobe Premiere. Before capture always make sure there is enough space in the drive saving to.  A clip that is 10 seconds long and typically have a size of 200 MBs.  

Note: 
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Once in Adobe Premiere the user could select to load a batch file created by p_vims.exe or setup video capture manually.  The file created by p_vims can be used by Adobe Premiere to make multiple captures at one time.  Under the File tab select Open and navigate to your batch file, <batchFileName>.pbl, and select OK.  This will open a Batch Capture window.  In the window there are two symbols worth noting; the star, (, on the left of each selection and red circle, (, on the bottom near right.  The star represents the selected track to be recorded and can be on or off by clicking on them.  Once all the tracks are selected click on the red circle, (, to begin the capture process.  Other than using a batch .pbl file capturing the video can be done manually.


To manually capture video once in Adobe Premiere open file tab and select -> Capture -> Movie Capture.  This will open the Movie Capture window.  There are three fields that need to be filled before the capture can begin; File Name, In, and Out.  Next to File Name: type in the name of the desired output file.  Next to the In: follow the same format, hh:mm:ss:ff, to designate the beginning of the capture.  Next to the Out: follow the same format, hh:mm:ss:ff, to designate the end of the capture.  To determine a good start and end time for a 10 second clip subtract 5 seconds from the annotator’s time code for the In field and add to seconds to that for the Out field.  Once the selection has been made select the Capture In/Out button.  This will open up a separate window with [image: image3.png]Load Project Settings:
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the clip just captured.  At this point the film needs to be converted into a Quick Time movie.


To convert the captured Premiere AVI into a Quick Time movie make sure the 

clip window is active (up front).  Open File tab and select Export Clip -> Movie.  This will open the Export Movie window.  Next to File name: type in just the name of the clip and not the extension.  If the Save in: is not the directory of choice Navigate to the appropriate directory.  Click Save and when done converting make sure the movie is viewable.  Converting after capturing with a batch file is the same and have to be done one by one.  
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