PIN ASSIGNMENTS FOR MCIL-6-MP

1
MOTOR POWER GROUND
2
+48 VDC MOTOR POWER
3
ISOLATED INSTR. POWER GND
4
+12 VDC INSTR. POWER
5
(5 V ANALOG CONTROL SIGNAL
6
0-5 V ANALOG SPEED OUTPUT
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DO NOT RUN IN AIR – FLUSH / FRESH WATER AFTER USE










