AUV Docking Project Meeting Notes

26 August, 2006
Attending: 

Brett Hobson, Thomas Hoover, Rob McEwen, Farley Shane, Jim Bellingham

Overview:

· Docking operations planned for Aug. 28, 31st, 5th, 7th – with RHIB, 
· Sept.12 with Zephyr an option
· Recover Dock (leave tripod) with Zephyr, Sept. 13th
· Clean up dock, repair and problems and redeploy in tank until Oct. 13
· Re-deploy dock Oct 17th
· Docking operations for approx. 10 days over 6 weeks
· Recover complete dock Dec. 4rd (Pt. Lobos)

· Clean up and decommission dock

· Finalize documentation by end of year

Tasks:

1) Spare RHIB computer
a) Re-attach Freewave Thomas
b) Disconnect UPS buzzer Thomas
c) Install Gaia to increase visibility  Thomas
2) AUV tracking

a) Mount transducer mount (dive ladder) Brett
b) Mount transducer Brett
3) Process accelerometer data from last trip to MRY Thomas
4) Register trailer  Brett
5) Compass
a) Confirm magnetic compass compensation routines are onboard MTi

b) Modify driver for Dorado MVC Rob
c) Remove CTD board set; repeat Thomas
d) If there is still large (<5 degrees) discrepancies, exchange Crossbow compass with old unit; repeat  Thomas
6) SSM comm. port
a) Investigate SSM A-comms for the following commands: abort, reset drop- weight, reverse thrust for 15 sec, forward thrust for 15 seconds
7) Power Transfer
a) Modify the existing battery charging program Rich
8) Future Dates

a. Sept. 7th AGU abstract due

b. Sept 12, 13 Zephyr days
c. Dec 4, 5 – Dorado Low-Speed Control
d. Dec 11-15th; AGU Fall meeting; SF 





















