Mission Log

13 March 2006

RF Ping running

Dropweight reset running

Battery cell volts 4.16, 4.15, 4.18, 4.16, 4.14, 4.14, 4.16, 4.16

TD new TailCone 
sat

TD crossbow
sat

TD parosci
sat

TD dvl
sat

TD gps
sat

fanTest press 64.0 kPa, temp 29.8/85.6, Hum 11.6
Launch at 0943
Updated tailcone calibration file

Running compass calibration CrossCal.cfg
1025  running surface_setpoint.cfg
1055 running OffshoreBox.cfg
Should surface NLT 1108

Surfaces 1105

Down loading data.  Set up OffshoreBox3x.cfg which will repeat mission three times with GPS surface at beginning and at start of each repeat.

1149 started OffshoreBox3x.cfg.  Surface NLT 1230.

1154 restarted OffshoreBox3x.cfg.  Surface NLT 1235.

1207 surface on first loop.  Mission abort due to operator error on mission timer.
Increased mission timer to 2400.

1214 restarted OffshoreBox3x.cfg. Surface NLT 1245

1223 surface on 1st loop.
1224 start 2nd loop.

1233 surface on 2nd loop
1233 start 3rd loop.

1243 surface

1245 started Outback.cfg.  Surface NLT 1301, expected surface is 1257. Get GPS fix and return to OboxNW, surface NLT 1315, expected surface is 1311.
1256 surfaced at NorthCompass waypoint for GPS fix.
1257 submerged for run back to OboxNW

1308 surface at oboxNW

1330 start InshoreBox.cfg
Aborted, reasons unknown

1335 restarted InshoreBox.cfg.  Surface NLT 1348.  Expected 1344.

1348 surface on timer abort.
1354 start InshoreBox.cfg.  Surface NLT 1408.  Expected 1405.

1405 surface.
1410 start InshoreBox7a.cfg.  Surface NLT 1428, expected 1420.
1421 surface
1430 start InshoreBox7as.cfg.  Surface NLT 1448, expected 1442.
1440 surface
1442 start InshoreBox5as.cfg.  Surface NLT 1500, expected 1454.

1446 re start InshoreBox5as.cfg.  Surface NLT 1504, expected 1500.

1459 surface.
Recovered onboard.
Plugged into tether.

Pressure switch turned off.

Unable to insert magnet due to strap.

On return to port, removed Tail Cone for transfer to CTD vehicle an inserted magnet to turn off batteries.
Left vehicle on R/V Zephyr over night, demobilized in morning.

Battery charge on return to shop at noon.

