Mission Log

30 March 2006

RF Ping running

Dropweight reset running

Battery cell volts min 4.16
TD new TailCone 
sat

TD crossbow
sat

TD parosci
sat

TD dvl
sat

TD gps
sat

fanTest not able to access
Launch at 1000
Ran RunOut.cfg to clear kelp bed.

2006.089.01 fail to start due to typo
2006.089.02 fail to start due to typo
Drifted into kelp, towed clear.

10:29 

2006.089.03

Ran RunOut.cfg to clear kelp bed.

10:36 surfaced at “safepoint” waypoint

Run “CrossCal-15.cfg”

2006.089.04 failed to start

Start 10:41

2006.89.05
Done NLT 10:46

Remarks: vehicle was porpoising for no apparent reason.  Rob is looking at data to determine what was causing behavior.
11:11
Run “box500-10.cfg”

2006.089.06
Surface at first corner

Done NLT 11:24

Timed out on mission timer, set too low.
11:36

2006.089.07 bad start

2006.089.08 running “box500-10.cfg”

ibox1 (NE) at 11:42

obox6 (NE) at 11:48

obox7 (NW) at 11:56
ibox2 (NW) at 12:04

Done NLT 12:15

12:20
2006.089.09 run “OutBack500.cfg”
Outback at 12:30

ibox2 (NW) at 12:36
12:50

2006.089.10 run “OutBack500.cfg”

Outback at 1257
ibox2 (NW) at 1304
1350

2006.089.11 fail to start

2006.089.12 fail to start
2006.089.13 fail to start
2006.089.14 run “OffshoreBox.cfg”
NLT 1405

1424
2006.089.15  Run “OffshoreBoxRev1.cfg” 
Surface NLT 1439
1439

2006.089.16 Run “OffshoreBoxRev2.cfg”

Surface NLT 1454

1453 on surface
1459

2006.089.17 Run “OffshoreBoxRev2.cfg”

Surface NLT 1514

1511 on surface
