Mission Log for 12 September 2006
2006-255-00 GoBack.cfg mission with destination of iboxNE

2006-255-01 InshoreBox.cfg mission with min altitude of 5 meters. Vehicle flew over dock. 
2006-255-02 InshoreBox.cfg mission with min altitude of 1.9 meters.  Vehicle docked, at 523 seconds into mission.  Video from dock:
11:10:41 Vehicle makes first contact with dock.
11:10:44 Hard Stop

11:11:00 Sliding in cone 

11:11:36 Vehicle in docked position.

2006.255.03 Undock.cfg mission with duration of 20 seconds.  Vehicle undocked and redocked.  Video from dock:
12:08:44 Prop starts spinning

12:08:52 Dock rocks back, vehicle starts to slide out

12:09:07 Prop stops, vehicle is still partially in the dock.

12:10:24 Prop starts spinning to push vehicle back in.

12:10:46 Vehicle slides into docked position.

12:11:30 Prop stops

2006.255.04 Aborted mission due to parosci failure.
2006.255.05 Undock.cfg mission with thruster duration of 25 seconds, end depth of 3 meters.  Vehicle undocks and transits to iboxNE.  Total navigation error is 16 meters south of GPS position on surface (16/395 =  4% error). Video from dock:
12:23:38 Prop starts spinning

12:23:39 Vehicle begins to slide back out

12:23:56 Vehicle is clear of dock.

12:23:57 Last view of prop, still spinning.

12:24:03 Vehicle lost from view backing toward surface.

2006.255.06 InshoreBox.cfg with minAltitude at 1.8 meters, speed during homing is 1.0.  Vehicle docked at 594 seconds into mission.  No video from dock yet.:
Should be 12:35 to 12:47

2006.255.07 Undock.cfg mission with thruster duration of 25 seconds, end depth of 3 meters.  Vehicle undocks and transits to iboxNE.  Total navigation error is 14 meters south of GPS position on surface (14/385 =  3.6% error). No video from dock yet.
Time line is not clear but should be between 12:47 and 13:17.

2006.255.08 Mission abort 13:17
2006.255.09 InshoreDock.cfg mission with minAltitude at 1.8 meters, speed during homing is 1.0.  Vehicle docked at 515 seconds into mission. Video from dock:
13:28:04 Vehicle makes first contact with dock.

13:28:14 Vehicle starts to slide into dock.

13:28:22 Vehicle slides into docked position.

2006.255.10 Undock.cfg mission with thruster duration of 25 seconds, end depth of 3 meters.  Vehicle undocks and transits to iboxNE.  Total navigation error is 14 meters south of GPS position on surface (14/387 =  3.6% error). .  Video from dock:
13:53:26 Prop starts spinning

13:53:29 Vehicle begins to slide back out

13:53:44 Last view of prop, still spinning.

13:53:45 Vehicle is clear of dock.

13:53:49 Vehicle lost from view backing toward surface.

2006.255.11 Mission abort 12:04
2006.255.12 InshoreDock.cfg mission with minAltitude at 1.8 meters, speed during homing is 1.0.  Vehicle approached dock to within 10 meters before homing behaviour timed out and vehicle headed for next waypoint.  Difference between this mission and missions 2006.255.06 and 2006.255.09 is vehicle received a wayward USBL hit early on and spent time maneuvering to resolve USBL contact.
2006.255.13 Mission abort 14:20
2006.255.14 InshoreBox.cfg with minAltitude at 1.8 meters, speed during homing is 1.0.  Duration for homing is 330 seconds. Vehicle docked at 571 seconds into mission.  Video from dock:

14:31:30 Vehicle makes first contact with dock.

14:31:34 Vehicle bounces off other side of cone.

14:31:39 Vehicle starts to slide into dock.

14:31:57 Vehicle slides into docked position.

2006.255.15 Mission abort 15:33
2006.255.16 Undock.cfg mission with thruster duration of 25 seconds, end depth of 3 meters.  Vehicle undocks and transits to iboxNE.  Total navigation error is 14 meters south of GPS position on surface (14/383 =  3.6% error). .  Video from dock:

15:36:46 Prop starts spinning

15:36:51 Vehicle begins to slide back out

15:37:05 Last view of prop, still spinning.

15:37:06 Vehicle is clear of dock.

15:37:09 Vehicle lost from view backing toward surface.

No more missions this day.
