This includes finalizing the design for the samplers, the mounting rack and the foam pack. Additionally, we will need to build a simple circuit board that will consist of a PIC and some high side power switches to trigger the samplers. Due to the large number of penetrations required, we can’t put our electronics in the main vehicle controller sphere. A small amount of software development will be required to trigger samplers and to read proximity sensors.

