Gulper Node Controller test sheet

Pressure:_______________

Cycle number: ___________

Other test conditions: ________________________________________________________________________________________________________________________________________________
1. Check software version


Inputs: Get Version command


Expected Results: ASCII version number


Version: ___________________
2. Get Status


Inputs: Get Status Command



Proximity: 0



Pin Puller: 0


Expected Results: 0000


Status: ______________________
3. Fire command


Inputs: Fire Command


Expected Results: Voltage pulse across resistor for ~300msec


Pulse length: ___________________

Voltage during pulse: ____________

Connect pin 10 and pin 11 of J2 to simulate proximity sensor within 30 sec of sending fire command.

4. Query Command


Inputs: Query Command


Expected results: query returns valid elapsed time between firing and pulling pin 
10 to gnd (pin 11) 


Time: _____________________

5. Get Status

Inputs: Get Status Command


Expected results: status = 0111


Status: ______________________

