Gulper 1/13/06 Meeting Agenda

1. Update

a. AUV tests:  4 dives, 3 triggering a sample

i. No sample validation due to cold induced pumping- need to build prototype with exact sized tubing.

ii. Some uncertainty on how long it took to fire

Mission 2005.299.12

Gulper fired at mission elapsed time of 13074.20

Mission 2005.301.00

Gulper fired at mission elapsed time of 14601.2 seconds

Proximity switch closure at mission elapsed time of 14604.0 seconds

Mission 2005.308.00

Gulper fired at mission elapsed time of 15018.2 seconds

Proximity switch closure at mission elapsed time of 15238.0 seconds (kinda of weird, a long delay)

b. Actuator:

i. Survived pressure tests to 6000 psi

ii. Larry built oil-comped housing

iii. Worked after sitting in cold room

iv. Wires damaged right before test on ventana, at manufacturers now to be repaired. may not provide enough force…

c. Mounting samplers in new AUV

i. Choices between 10 x 1.9L samples and 12 x 1.07 L samples.

ii. Need to order foam pack ASAP

iii. CDR for foam pack asap.

