Gulper Meeting Notes June 15, 2006

1. Oceans paper

 An outline was passed out; each section was assigned to one member of the group. People will have their sections to Alana by July 5.

2. Sample testing on the AUV CTD

The CTD vehicle will be going out in 2 weeks. We will pull the lisst and mount the gulper as we have in the past. Hans thinks there will be time to code up a fluorescence based trigger event. If not we will revert to triggering at a given depth. We will test the samples salinity and John will do microscopy on the sample if we do use fluorescence as a trigger.
3. Integrating a sampler for the summer field program

Farley is going to work with Hans to figure out how to include at least 1 sampler in the AUV with the Lisst. This might require modifying foam or the plate onto which the Lisst mounts. We will try to have the Gulper mounted by our July 31 Zephyr ship days. Then leave the sampler in through the August field programs. We decided that integrating the larger pin puller was a lower priority, but would be nice if we got everything else in place.
4. Mechanical Critical design review

We are waiting for 2 more salinity data points for the ROV sampler tests, if both correspond to the vehicle CTD, then we can confidently schedule the mechanical CDR. I expect we will have these results in the next couple weeks. The electrical CDR will have to wait until after I return from my August cruise.

