Preliminary design requirements for ocean water sampling users:

	Lab
	Z Resolution
	# Samples
	Sample Volume
	Environment
	Processing
	Comments

	 
	 
	 
	 
	 
	 
	 

	Kolber
	1m
	20-40
	20 mL
	200m
	native
	Low cross talk,

	 
	 
	 
	 
	 
	 
	contextual info: NOSA

	 
	 
	 
	 
	 
	 
	 

	Haddock
	1m
	20
	.25-2L
	200m
	particles, preservation
	replicates, contextual: fluro/lum.

	 
	 
	 
	 
	 
	 
	 

	BOG
	1m
	50
	2L
	200m
	particles, preservation
	split samples for multiple assays

	 
	 
	 
	 
	 
	 
	 

	Chemistry
	1m
	50
	20-30mL
	200m
	native
	chemical compatibility

	 
	 
	 
	 
	 
	 
	 

	Vrijenhoek
	1m
	10
	5-20L
	200m
	particles, preservation
	 

	 
	 
	 
	 
	 
	 
	 

	Microbiology
	1m
	25
	50mL-4L
	200m
	particles, preservation
	need prefilter

	 
	 
	 
	 
	 
	 
	 


