Gulper meeting Mar 9, 2007

Attending: 

Zephyr ship days, engr. test: March 19 (CTD) March 21, 22, Apr 3, 4, 

Zephyr science test days: April 10, 11 (Vrijenhoek/Jones) Apr 26, 30 (24), May 2, 3 

Operational: 
1. March 21,22 we will run the C1M1C1 mission, taking 3 sets of samples from max depth to shallow.

2. Will try to integrate with vehicle Thurs and Fri of next week.

3. How do we identify which sample is which

4. How are we going to handle all the water- 

a. For science test ‘the responsible scientist will do with it what shall be done’

b. Cleaning will be the responsibility of the scientist

c. For engineering tests, develop a little dispenser tool

Mechanical:

1. Seat belts designed for samplers-done

2. Jim is assembling the samplers, expect finished mid-next week
3. Waiting for handle springs- not necessary for testing

4. Larry working on the linkages and the sampler cables

5. Need to modify foam on top of battery

6. Modify foam above samplers

7. pistons modified to take two springs- done

8. Ti nuts on shaft need to be modified

9. seals are all in – we will test the square seal on the ROV

10. brackets that hold the hall effects are being anodized
11. Need to mount burn wire mechanism and add drain holes- done
12. Do we need a plug on the back of the piston to relieve the pressure- need to talk to Chris about whether we need it

13. Need to replace stainless hardware in sampler with Ti

Electrical:

1. Reprogrammed node controllers to have a reset- need to reprogram node 0 
2. need to buy more impulse cables

3. need to install hall effects, when brackets get back

4. Jim potted the hall effect cables, we only have 9
5. Jose is potting pin puller cables today-done
Software:

1. Rob is working on a driver, a ‘arm the gulper’ behavior as per Hans’ directions

2. Fred will work with Rob, the behavior is very similar, and will talk to John next week to explain the clustering algorithm and if it is a good match for him.
