Gulper meeting Mar 23, 2007

Attending: 

Zephyr ship days, engr. test: April 2, 3, 4,10 

Zephyr science test days: April 11, 12 (Vrijenhoek/Jones) Apr 26, 30 (24), May 2, 3 

Operational: 
1. April 2,3 we will take 3 sets of samples from max depth to shallow.

2. Will try to integrate with vehicle early next week.

3. How are we going to handle all the water- 

a. For science test ‘the responsible scientist will do with it what shall be done’

b. Cleaning will be the responsibility of the scientist

c. For engineering tests, develop a little dispenser tool

Mechanical:

1. Jim is assembling the samplers, done except springs
2. Larry working on the linkages and the sampler cables-done
3. Need to modify foam on top of battery-done
4. Modify foam above samplers-done
5. Ti nuts on shaft need to be modified

6. we will test the square seal on the ROV- no dice
7. brackets that hold the hall effects are being anodized-done
8. Do we need a plug on the back of the piston to relieve the pressure- need to talk to Chris about whether we need it

9. Need to replace stainless hardware in sampler with Ti-done
10. remake proximity sensors

11. need bracket for j-box

12. threaded rod for foam pack needs to be stainless

13. polish triggers

14. holes for AUV cabling

Electrical:

1. Reprogrammed node controllers to have a reset- done
2. need to buy more impulse cables-done
3. need to install hall effects, when brackets get back-done
4. Jim potted the hall effect cables, we only have 9 will make more when cables arrive
5. New pin puller housings are here, will plan a switch out after May dives (looks like we have a window in June)
Software:

1. Rob is working on a driver, a ‘arm the gulper’ behavior as per Hans’ directions

2. Fred will work with Rob, the behavior is very similar, and will talk to John next week to explain the clustering algorithm and if it is a good match for him.
