1. Rover_Tether.tif: This is an image from the Rover “Tether Cam”. The camera is mounted on the aft of the Rover and enables us to watch how the tether unravels from the cable mandrel as we drive away from the MARS node. An adhesive binds the cable to itself. Larry Bird designed and built this portion of the system.

2. Fluoro_1247…: This image was an accident but pretty neat.

3. Port insert: a low-res frame grab from our chamber video cameras, shows the port respirometer immediately after it is inserted.

4. Port after: A second frame grab taken of a respirometer prior to removing it from the site.

5. Transit_12472…tiff: This image is taken from our transit camera (illuminated by a 250 W-sec strobe). We take images every 1 meter while driving between study sites.

6. Transit_12476…tiff: A couple of hag fish and a rock fish are captured in another transit camera image.

