Frame Grab Descriptions

1.Lobos_frameRover: Viewing the Rover from above prior to connecting Rover to MARS.

2. PickingupSiim: Pilots D.J. Osborne and Knute Brekke used the vehicle manipulators to pick up Rover Siim and cable bundle. Ventana carried the Siim and cable from the Rover to the MARS node approximately 45m away. 

3. PlugInRover: the Rover ODI connector is being plugged into the MARS node.

4. RoverTether: We flew over the Rover tether to inspect that is was nicely laid out.

5. BlueLightSpecial: Two blue lights, located on the front and aft of the Rover  are used to provide illumination to image the sediment and the cable pack.

