Benthic Rover BaseStation Application

1.	GUI application used to remotely interact with the Benthic Rover during deployments. 

2.	Intended to replace HyperTerminal as the acoustic modem front-end user application.

3.	Functionality
a.	Rover status displayed and maintained in a GUI window
i.	 Active Mission
ii.	 Phase
iii. Site number
iv. Incubation progress
v.	 Mission timer
vi. Heading
vii. Current data
viii. Battery level
ix. Modem battery level
b.	Basic mission control
i.	 Stop mission
ii.	 Start new mission
iii. Download mission configuration file