O-Ring List for Benthic Rover

Description



part number
 qnty/assy
total qnty 

Drive Motor


Tube seal


2-251

2


Shaft Seal


SKF9811 LipSeal
1
2

Motor Amp (EZ Amp)


Tube bore seal


2-041

2

4


Tube face seal


2-042

1

2 *two motors


Feedthrough 


2-112

2

4 * two motors


Subconn BH10M face

2-015

2

2

Spheres


Face seal – outer

2-282

1

2


Face seal – inner

2-283

1

2


MINM face


2-023

6



MINM bore


2-020

6

MINM bore 2


2-019

6



MINK face


2-019

14



MINK bore


2-016

14

MINK bore 2


2-016

14


MINK CCP bore

2-016

17


MINM CCP bore

2-019

6



Overpressure face 

Rack Motor


Tube Bore


2-141

1

2

Optode


Body top face


2-020

1

2


Base bore


2-028

1

2


Thermal Sleeve

2-118

1

2

Stirer


Base Bore


2-030

1

2


Top Bore


2-133

1

2

Valves


Piston Floating 

2-334

1

4


Rod – Reciprocating

2-112

1

4

Pressure Relief Valve



SAE



3-904

1

3


Face



2-015

1

3

Iridium beacon


Bore



2-231

2

Argos beacon



Face ?



218

2

