+12V Converter Assignments
Converter 1: 12v, 25W

1. Chamber cameras (2), Insite Nova model, 12v, 175 mA,  2.1 W per camera 

2. Optodes (2), Aanderaa 3830, 12v, 80mA, 1W per optode

3. Valve pumps (2), Seabird SB5, 12 v, 0.95 A, 11.4 W per pump
Converter 2: 12v, 25W

1. Video Server, Axis 241, 12v, 8 W max

2. Clean Pumps (2) , SeaBird SB5, 12 v, 0.95 A, 11.4 W per pump

3. Transit Camera, Prosilica

