RTC3000
 

12Vdc -> draws 90mA
24Vdc -> draws 50mA
 

 

RTC4000
 

24Vdc -> draws 54mA
48Vdc -> draws 20mA
 

The measurement above is taken without using any I/Os and with amplifier off. 
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