Rover meeting notes October 6, 2009
Rich, Paul, Ken, Alana
Rover deployed on MARS October 1, 2009. So far all systems are working. Including the new strobe.

MARS goals:

1. Run multiple missions without intervention

2. Test sleeping after it has been working 1 month

3. Test new strobe

1. Software

a. Integrate new sleep mode with Tri-M power supply

i. Save state- making more progress

b. Reset current meter to sample every 6 sec

c. Sample optodes during insertion

d. Sample optodes for 2 min during incubation

e. Only move into favorable current

f. Get change list for EZServo firmware- Paul

g. Turning 

h. Record current meter data- done
i. Error management- no progress

j. Matching SSDS upload template 

k. Upload current data on SSDS 

l. Add metadata to transit images

m. Autonomous software

2. Electrical

a. Order another HESC-SERD

b. Wire SD line of Tri-M to modem- will have to wait
c. Check out options for external hardware watch dog timer (Paul)

d. Rev load controller (Paul)

i. Over current still not working- progress

ii. Final configuration of connectors- progress
iii. Load current quit working- fixed
iv. Captured changes in orcad- new folder load controller main

v. Started designing carrier board

e. Redesign chassis to include load controller 

f. Design long term battery pack (Paul)

i. Hand off to Jose

g. Build up second battery sphere- Alana
h. Cabling between battery spheres- Alana
3. Mechanical

a. Change F-stop on camera- set to F16 maybe, 1 above 11
b. Chamber cleaner

c. Corrosion on stand alone modem-done
d. Plastic cover for spheres

4. Science

5. Long Term

a. need to spend out money by the end of year

