Tasks

1. Test

a. Wake up line

b. Rack and prop motors- all functions

c. Sediment switches

d. Optodes

e. Transit camera and strobe

f. New position of tether cam light

g. Web relay functions

2. Software

a. Integrate new sleep mode with Tri-M power supply

i. Make sure we can talk to the board- done

ii. Test shutdown command

iii. Test start up in N seconds

iv. Set polarity of ign input to active low, use windows program

b. Get change list for EZServo firmware

c. Error management- no progress

d. Matching SSDS upload template 

e. Upload current data on SSDS 

f. Add metadata to transit images

g. Autonomous software

3. Electrical

a. Separated port and stbd rack motor serial port-done

b. Routed stbd optode to second serial port-done

c. Need to check that serial ports are jumper activated

d. Removed all ezservos and sent to all motion for firmware upgrade-done

e. Added 2port web relay to batt sphere

f. Test new cables for optodes

g. Make sure wake-up line is wired in cable

h. Need to check trans cam cable long enough then pot

i. Power web relay from deck cable as well as mars

j. Make Rich a push button switch

k. Rewired optodes to meet new mbari standard- done

l. Sent cables to subconn for splicing back in 2 weeks

m. Put new antennae on RF and argos beacon-done

n. Check Tri-M serial port connected properly- done

o. Buy 2 more EZServos

p. Burnwire needs to be switched 

q. See about changing LEDs for nova camera

r. Check out options for external hardware watch dog timer (Paul)

s. Rev load controller (Paul)

i. Gf working- done

ii. Voltage and current sensing working –done

iii. Over current still not working

iv. Final configuration of connectors

t. Redesign chassis to include load controller 

u. Design long term battery pack (Paul)

v. Build up second battery sphere

w. Cabling between battery spheres

4. Mechanical

a. Sediment switch alignment

i. Fix broken sediment switch

ii. Lock sediment switch

b. Need to mount argos

c. Need to check if oil got into the current meter housing.

d. Fix port rack motor issues

e. Make new cap for port rack motor was cracked in recovery

f. Motor housings being modified to allow access to the the 1 atm housing without opening the oil filled side

g. Need to reassemble housings and recomp all four comps

h. Need to reattach racks

i. Need to remount optodes

j. Need to fix scales- etching damn it!

k. Make cable keeper reversible

l. Need to mount new strobe

m. Need to repackage transit camera- must clean lenses!

n. Tilt tether cam light up

o. Chamber cleaner

p. Corrosion on stand alone modem-why?

5. Science

a. Calibrate optodes

