Tasks

1. need to spend out money by the end of year

2. Test

a. Wake up line

i. Ign connected to the web relay

ii. SD for modem

b. Rack and prop motors- all functions

c. Sediment switches

d. Optodes

e. Transit camera and strobe

f. New position of tether cam light

g. Web relay functions

3. Software

a. Integrate new sleep mode with Tri-M power supply

i. Test shutdown command

ii. Test start up in N seconds

iii. Set polarity of ign input to active low, use windows program

iv. Save state

b. Get change list for EZServo firmware- Paul

c. Error management- no progress

d. Matching SSDS upload template 

e. Upload current data on SSDS 

f. Add metadata to transit images

g. Autonomous software

4. Electrical

a. test port and stbd rack motor, and second stbd optode serial port-Need to check that serial ports are jumper activated
b. Address the ezservos before remounting

c. Removed all ezservos and sent to all motion for firmware upgrade-done

d. Added 2port web relay to batt sphere

e. Add to pre-dive to tighten current meter

f. Test new cables for optodes

g. Make sure wake-up line is wired in cable-done
h. Need to check trans cam cable long enough then pot

i. Make Rich a push button switch

j. Burnwire needs to be switched switch wires not burnwire
k. Check if camera can be adjusted

l. Add rover name to connector

m. Check out options for external hardware watch dog timer (Paul)

n. Rev load controller (Paul)

i. Over current still not working

ii. Final configuration of connectors

iii. Load current quit working
o. Redesign chassis to include load controller 

p. Design long term battery pack (Paul)

q. Build up second battery sphere

r. Cabling between battery spheres

5. Mechanical

a. Sediment switch alignment –johnny in progress
i. Fix broken sediment switch

ii. Lock sediment switch

b. Need to mount argos -done
c. Need to check if oil got into the current meter housing-done, not in housing

i. Not sure where the oil went

ii. Recomped it

iii. Needs to be tightened, will watch over the weekend

d. Fix port rack motor issues

e. Strain relief

f. Make new cap for port rack motor was cracked in recovery

g. Motor housings being modified to allow access to the the 1 atm housing without opening the oil filled side- done
h. Added vent on drive motors -done

i. Need to reassemble housings and recomp all four comps

j. Need to reattach racks

k. Need to remount optodes (calibrate first)
l. Need to fix scales- etching damn it!

m. Come up with a cable restrainer for deployment
n. Need to mount new strobe

o. Tilt tether cam light up

p. Chamber cleaner

q. Corrosion on stand alone modem-why?

6. Science

a. Calibrate optodes

