Rover meeting notes Nov 12, 2009
Rich, Paul, Ken, Alana
Rover deployed on MARS October 1, 2009. So far all systems are working. Including the new strobe. Will recover Dec 18.
MARS goals:

1. Run multiple missions without intervention

2. Test sleeping after it has been working 1 month

3. Test new strobe

1. Software

a. Integrate new sleep mode with Tri-M power supply

i. Save state- making more progress

b. Reset current meter to sample every 6 sec- you can’t
c. Sample optodes during insertion-done
d. Sample optodes for 2 min during incubation- changed to 4 min
e. Only move into favorable current- done
f. Get change list for EZServo firmware- Paul

g. Can we decrease current cone to 90 degrees

h. Turning 

i. Error management- no progress

j. Matching SSDS upload template 

k. Upload current data on SSDS 

l. Add metadata to transit images

m. Autonomous software

2. Electrical

a. Order another HESC-SERD- 
b. Wire SD line of Tri-M to modem- will have to wait
c. Check out options for external hardware watch dog timer (Paul)

d. Rev load controller (Paul)

i. Brass tacks?@##$%

ii. Over current still not working- done
iii. Final configuration of connectors- progress
iv. Started designing carrier board- pdr stage
e. Redesign chassis to include load controller 

f. Design long term battery pack (Paul)

i. Hand off to Jose

g. Build up second battery sphere- Alana
h. Cabling between battery spheres- Alana
3. Mechanical

a. Change F-stop on camera- set to F16 maybe, 1 above 11
b. Chamber cleaner

c. Corrosion on stand alone modem-done
d. Plastic cover for spheres

4. Science

5. Long Term

a. need to spend out money by the end of year

