Tasks

1. need to spend out money by the end of year

2. Test

a. Wake up line

i. Ign connected to the web relay- done

ii. SD for modem- next

b. Rack and prop motors- all but Port rack

c. Sediment switches- NP

d. Optodes – Jake is calibrating

e. Transit camera and strobe- done

f. New position of tether cam light

g. Web relay functions- done

3. Software

a. Integrate new sleep mode with Tri-M power supply

i. Test shutdown command

ii. Test start up in N seconds

iii. Set polarity of ign input to active low, use windows program -done

iv. Save state- making progress

b. Get change list for EZServo firmware- Paul

c. Turning 

d. Record current meter data

e. Test new rack software

f. Error management- no progress

g. Matching SSDS upload template 

h. Upload current data on SSDS 

i. Add metadata to transit images

j. Autonomous software

4. Electrical

a. test port and stbd rack motor, and second stbd optode serial port-Need to check that serial ports are jumper activated

b. need to set strobe power

i. start at max

c. Address the ezservos before remounting- done

d. Add to pre-dive to tighten current meter

e. Test new cables for optodes

f. Need to check trans cam cable long enough then pot-done

g. Burnwire cables need to be ziptied

h. Check if camera can be adjusted

i. Add rover name to connector- Paul

j. Check out options for external hardware watch dog timer (Paul)

k. Rev load controller (Paul)

i. Over current still not working- progress

ii. Final configuration of connectors

iii. Load current quit working

iv. Captured changes in orcad- new folder load controller main

v. Started designing carrier board

l. Redesign chassis to include load controller 

m. Design long term battery pack (Paul)

n. Build up second battery sphere

o. Cabling between battery spheres

5. Mechanical

a. Sediment switch alignment –johnny in progress

i. Fix broken sediment switch

ii. Lock sediment switch

b. Need to change batts on all beacons

c. Need to check if oil got into the current meter housing-done, not in housing


i. Not sure where the oil went

ii. Recomped it

iii. Needs to be tightened, will watch over the weekend

iv. No oil over weekend, it is a mystery, is back on vehicle

d. Camera housing: found corrosion between glass flat port at 17-4 statinless steel ring, as well as between ring and Ti housing. 

i. Will replace ss ring

ii. May not get parts before dive 

e. Fix port rack motor issues- done

i. Gear box broken when hit during recovery, replaced gear box

f. Strain relief around SIIM can -done

g. Make new cap for port rack motor was cracked in recovery- done

h. Recomp rack comps-

i. Need to mount port rack

j. Need to remount optodes (calibrate first)

k. Need to fix scales- etching damn it!

l. Come up with a cable restrainer for deployment- done

i. We will use tape

m. Need to mount new strobe

n. Tilt tether cam light up

o. Chamber cleaner

p. Corrosion on stand alone modem-why?

6. Science

a. Calibrate optodes

