
	20 Jan 2016

	World according to Henry
	Arctic proposal is in
Megafauna in Rover chambers. Data files are UTC. File name is local time. Chambers with animals not always associated with high SCOC 

	Larissa
	Data collection to start in Jan 24ish. 2 yr starting now. 

	To do
	Current meter repairs after Jan 1 they will honor quote
Order more re-enterable after cruise- Johnny to do
FIND Color plate- got image from Kathy- still no reply from Kathy- Not in N. side cabinets of test tank 
Battery schematics ALANA and PAUL- so much progress. In touch with Electrochem. Ask in Jan
Current vs archive Make for Camera tripod and Rover Folders- PAUL, ALANA, RICH. Ask in March

	Budget
	Weights for JOHNNY in Jan. Ordered 1300 and change for four weights.

	Pulse 66 Cruise debriefing
	PAUL- Waiting to hear back from Joe Borden. Time to check in

	Rover 
	Axis video server- Alana and Rich will test. Ask after maternity leave
ALANA to check on Argos beacon shipment
RICH ADD serial number to optode data files each line of cys log and csv files. Jpgs split into many pieces and so far can’t be reconstructed. Rich to try another method. Add data to project library and explain situation. Worth analysing and using mean insertion depth? 
Cameras spares: what’s new? Nothing. Ask after maternity leave
Strobes: ALANA has a spare but there is a pressure cycling issue10K lantern shark? Needs testing. Alana made all cabling. Test in pressure tank. Remind in Feb-March.
Assess all spares in Jan
Check optode 801 and connector ALANA. Feb

	Optodes
	Crissy to assess all optodes and spare parts

	Grab resp
	CRISSY. Are they in the same port? What’s the same on these? Plug each one into serial port (with power). Check both loggers to see what’s going on. Unplug optode and see if it’s sending a dummy number. Run optode sitting on bench. Take pics. Check SN of ones that worked before to verify is these have worked in the past (Henry here next week). CRISSY TO DO

	SES
	In future should put an argos on it
TS 7250 we own two but they are not identical but they could be spares. Should RICH set up that spare? Yes. So will have spare processor, camera- just ordered. Rev A was first one but didn’t do what it says. Got new board Rev B.

	New battery housing endcap-Alana and Johnny
	Have all connectors, have to decide where to put them. Have connectors, proceed cheaply- too successful elsewhere 
Johnny can work on chasis for batteries. Plan for mounting strobes and ballast.

	Snappy software-Rich
	Alana- Test with new camera. Needs to setup LEDs. The Rich will do the software. Hand over to Rich probably week of Jan 25.

	LED lighting-Brett
	Brett and Paul will test the brightness and flash duration. Fasteners and connector not Ti, need to be changed. 

	Scanning contract-Crissy
	They have all tripod film. QC, uploading, organizing. Camera sled in 2016. CRISSY TO QC

	Multibeam data
	Talked with Kelly, preparing paper for DSR because not calibrated

	Near Field camera
	1. That’s its name (NFC)
2. PAUL to see if camera fits in housing
3. How do battery and camera fit?
4. Check cables to lights
5. Have answers about which housing
6. Need to bench test two cameras firing on same strobe.
7. Tom to make a splitter cable. Get optos for real test. Make sure two cameras triggered by optoboard

	Manuscripts
	8. SES paper- Fluorometer standard. On track to finish this by Nov? Table inserted. Paul re-writing intro to compare to Carbon flux explorer
9. PAUL to send CRISSY link of SES images. Crissy to annotate images in VARS and get surface area. Somewhere in Project library
10. Station M modelling- Kathy incorporating comments
11. SCOC paper almost done

	June camera tripod deployment
	12. Contact Chris Grech about mob and demob, schedule grove crane- DO AFTER PRACTICE TRIPOD FRAME DEPLOYMENT. Better to go over port side. Need ROV on both days.
13. [bookmark: _GoBack]Talk with Craig Dawe about going up to look at camera tripod with ROV
14. June Precruise- make sure ROV is on there
15. Sediment trap 10-15 meters above camera tripod
16. Set up meeting with Chris Preston and Colleen
17. Adina Payton wants samples for carbon. Come down and we’ll talk

	Camera tripod 
	Bathysnap- own housing? How to synchronize? Remote shutter, give it long exposure time.
Get Brett to test fit of camera.
 We don’t know if we can get another camera from her. Just use our system
Test deploy it at MARS
Think about options
Get from Jen- specs of Bathysnap- height, type and angles of camera and strobe, type of camera, port, etc. Any spare parts we can use?? Test it in June (Carson dates). Alana
Concern about old benthos film cam housing is whether we can align camera with port, based on diameter. End cap of housing does not come off. Slave camera so only use one strobe, remotely. No intelligence needed in second camera. Can’t use just light to trigger because it would require the camera to be on all the time. ISOLATE so if Bathysnap floods it’s not a problem. Revisit after 1st of year. Better to have both cameras the same. Wait and test 

	Deploy camera tripod in June
	Ken and Alana to meet with Aaron Gregg on Jan 19th at 9am.

	Personnel schedules
	Paul and Johnny taking off as often as possible
Alana- out of office May, June, July. Work from home Aug. Should be back in 3 days  week starting Sept.



