	26 April 2017 

	VARS
	UTC to Local

	2018 proposal
	Smarten SES?
Rigging for sampling at 600 m
Spare sediment trap guts	
Frame with two releases
Pressure testing for one spare

	Fluorescence cams on tripod
	Budget for most expensive option…Proslica with stack. Is there room in FF camera housing? Possibly. Need main processor card with Ethernet, Newer version of Technologic. Maybe snappy can put that to sleepy-wakey. And light, deep sea power and light housing x 2. 2 bulkhead connectors/cables. 

	Argos beacons
	Which ones do we have, and on what? We should have three more sitting somewhere. New-Solo, SES, Old-Rover, 3 new and 2 old in lab. Put new one on Rover and Dualie. Need mounts for new style beacons for Dualie mast and mount for Rover

	Wave glider
	Establish single point person for each team

	Current meter
	Johnny to spec costs of getting current meter up and running. March not realistic. Johnny sent them to RDI. ~450 per to get inspected

	Core extruder
	Nov. Bring up in mid May

	Pulse 68
	Crissy to give Ken moorning drawings
Print hard copy of sediment trap bridles

	Sediment traps
	Spare guts- 6K tax and shipping for two sets. 6-8 weeks delivery time

	Rover 
	Sharpen port chamber cam focus. The company can change the resistors/current of spare. Then we’ll swap the spare if it looks good in Nov.Submitted. Rotate those cameras 
10K lantern shark. Pressure tested when sent five years ago. Test it at sea. Remember in September/October.
Don’t need to get oil filled ducer. Try to contact Rover before picking up. If can’t contact on LF consider swapping 

	LED lighting-Brett
	Check with Brett about getting a release

	SES
	Rigging for sampling at 600 m

	Dualie
	Two new pressure tested strobes. Done

	Scanning QC
	RICH- can you help with renaming script? For us, yes
Danelle
Start trying it out

	Manuscripts
	1. Kathy’s multibeam paper- Submitted in next week
2. MBARI anniversary issue. Station M – what engineering and science advancements have been made. Due in May
3. [bookmark: _GoBack]Create drop box folder with images

	Multibeam M
	This summer

	Jerseys
	Camo PULSE shirts. Stripe for each PULSE cruise. Full jumpers with tassels.  Eric will help with design

	Personnel schedules
	



 
 Dualie to do list
1. New spar buoy that’s weighted correctly with proper bracketing
2. Still have plenty of rings and shackles 
3. Both Knute and Marko are looking at how to release the tripod with the ROV if needed
4. Check releases for corrosion in Nov
5. Isolation was checked on everything with digital multimeter
6. Rings were put in bottom of bridles of sediment traps for recovery
7. Argos beacon will go on next time
8. Which guts are in the RF beacon 
9. Crissy to add a spot for tripod strobe hard-hat SN on deploy checklist
10. Need more freeweights. Get another full palette
11. Give bridge the RF freq so they can listen for sink time.
12. O rings for the current meter and isolation tape/heat shrink. Get same for Rover
13. Get homers for both camera tripods from Conway
14. Add to deployment sheet which camera system it is
15. Spare sediment trap controllers
16. Chinese fingers on SES drop-weight
Monocam to do list
1. New weight emergency release so pilots can release mooring. Is pin system viable?
2. Aquarium fish nets for getting small stuff out of samplers
3. More 5 gallon white buckets- carry at least five with us. Check the van
4. Buy 50 ft of galvanized long-link chain (1/2”) and galvanized shackles (10 of 5/8” and 10 of ¾”) 
5. More lugs for benthos releases
6. Modify drawing for SES depoymet
7. Modify existing mast assembly replace the one on the dualie. Make a new top from the one that’s on the deck
8. Dual camera tripod spar doesn’t have an argos. We need it to have one. Need clamps.
9. Homers for dualie. Get two from Conway. 
10. Troublshoot chamber optode from grab resp
11. Wake up call to be more careful in rigging lines, especially in calm weather.
12. Oversize 11/16 carbite remer for camera tropod
13. Buy more anodes. Make sure they are packed individually in plastic bags. 
14. Drill out all release anodes before we go to sea.
15. Needs more bolts for acoustic releases
16. Release o-rings
17. More huge kim wipes
18. More shoulder bushings for camera tripods
19. Software for running current meter data. Try to look at it today. 
20. More freeweights. 
21. More falcon tubes
22. Widemouth jars plastic UN certified
23. Better 37% formaldehyde and more borax to sea
24. Second coring station
25. Two sets of top clamps for spar buoys
26. Ballast weights need four. 
27. Iversen’s bio-op camera, then it goes into a gel.
28. Rob Young- what do you really want?
29. Rob’s student (female) might come

