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	Rover Pulse 70
	One sphere worth of new Rover batteries in case of disaster. (4 PACKS)
Alana to give Crissy # of Rover packs and cam tripod lithium packs in stock.
Swap out calibrated optodes (2).
Give optodes that were good in the grabs
Release mechanism
Fried pin is the ground pin
LF modem head- get an oil filled if we get another one. Troubleshoot corrosion
Paul ordered LF battery

	SES
	Incorporate fluorescent puck? Biofouling?
Teting over weekend- 9 min per sample, got to 600 samples, no errors.
2 hr no pass through
Repeat calibration in test tank, add fluorescent puck

	Pulse 70 batteries
	Alkalines

	Lasers
	Need to know tilt and altitude. Precise but not accurate.
Need cables. Buy Medusa.	

	CTD
	Goldberg at Seabird- SBE37SMP has pump, recorder, can be set up to work at specific times, totally independent $8300 in titanium housings. Moos project has them. Rover has CTD so we can check that to see if temp has actually changed. Rover oxygen event

	Optodes
	Ask about calibration. Calibrate more often
NEED TO CALIBRATE- track down equipment from Lovera
Update optode list- add deployments
STBD- Chamber 296
STBD Reference 799
Port Chaber 961
Port reference 289

	SCOC
	Revisit slope adjustment. Crissy get on project library Rover deployments

	Dec Cruise
	Ken and Alana talked with Jim. Jim checking with collaborators- Looks promising- Do something nice

	Castroville
	Take cam sled apart, put in pallet and put on top of van
Would Francois want the benthos pop up bucket buoys (x3). Waiting for facilities to move cam sled here.

	Wave Glider
	Everything worked

	Camera tripod
	Lots of testing. Alana thinks the anywhere USB is old and causing communication problems. Could be hardware incompatibility. Went through four different machines and all have issues. Anywhere USB power plug is on outs (but fixed). Need to get newer hardware. Got new Anywhere USB and similar. Worked.

	Project update
	Ken to pick dates.
Update of how the technology we’ve developed can be used in other places, future. Next Wed work through it.
Engineering acomplishments so far: Rover, SES, Dualie, + 1 yr deployment. Refresh what the instruments do. We’ve overcome these challenges (including turnover in less than 48 hr). Drew’s time lapse of clearing the deck. Next steps- event triggering (on sea floor, profiling). Getting a better picture of the pulses. This technology doesn’t need to be used only at Station M. Kathy is interested in building a Rover.
Show the science of how this fits into the bigger picture. Methods. Science, Future. 
Alana- big picture why is this scientifically important
Tech roadmap, strategic plan.
Fast sinking events, integrating carbon budgets supply/demand, high res long-term sampling
Next lab meeting have this thing flushed out.
Viper after SES from abstract presentation
End on video transects, Introduce Laser measure and ultimately go to AUV transects and Park and Fly

	Manuscripts
	[bookmark: _GoBack]Surface to sea floor in revision 

	Larissa’s MS
	Spatial distance data organization

	Open House
	July 21st

	Multibeam M
	Next summer ?

	Personnel schedules
	Ken out 17th, out 2-3 weeks
Rich will be out April 9 - 12, the entire week before we mobilize for the April 18-24 cruise.
Crissy out 15-31 July



Ordering:
Wish list
Seaconn connector for replacement of bad pin cable
CTD 8.3K
Figure out what cable needs to be replaced
Ti seaconns
Anywhere USB

