	9 October Sept 2019

	Lasers
	Hang up is mount. If we have angles, Johnny can make the mount. Working on getting the laser mount done.
Need to calibrate Tueday on shore. Ship gets back today 1900

	Mooring failure
	Ready to go except for new anchors for elevators
Hardware is in. All tested except for galvanized. 

	Upside down sediment trap
	Cups are finished. Need to put union on cups.

	Larvae pump
	Larval pump is in the tank testing!!
Getting wet weight
Goes through a lot of power waiting. Has no standby sleepy.

	Wave glider
	Getting ready for Canon. Tiny going to station m. working. Leaving by tomorrow am. Connes working great.

	Macro system
(aka shrimpoteuthis)
	Don’t ask till after cruise
Sidelined until the other aspects are done. Keep up momemtum and finish after cruise.
50 mm lens, higher contrast. Cut housing in half
Will we have a pointer laser ready?
Lid’s coming in the mail.
Johnny working on endcap. 
Test in dark
In 2020 Change to easier to use menu? Engineering logging?
To measure angle off horizontal- ~30 degrees. Move to 45. Mount battery at mud level. 
No purge port, use alkalines for lasers
Pressure test? Pump helium in to test weld?

	Cruise prep
	Bring doubles of lines
Alana inventory, packing Monday the 7th. 
Mooring lines are in buckets. Ready to deploy except for hardware.
Add beacons to rescue float pack. Strobes and VHF. 
Nitrogen bottles- Johnny – we have plenty for the cruise.
Spar buoy fixes- get batteries on instruments
Crissy sediment trap controller batteries
ADCP put battery in
ADCP base.
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	Solo camera height, angles
	Not coming back. New mooring line will go on Solo camera and two inverted traps. 

	30 year volume
	Foram paper has been published

	Olmo
	Revising draft. Resolve field of view discrepancy 

	Personnel schedules
	Rich-Sept 19-4 Oct
Alana- 9-17 October



