	18 Sept 2019

	Lasers
	Dan is coming to talk about helical arrangement: decide on mount configuration and target 
Duane has put Dan’s code on version control in GIT 
Looking for bodies to sit down and do frame grabs/measurements.
Before cruise- need to set angle of lasers and get helical twist.
Make new is situ calibration target with shades of gray and put colors in there.
Talking mounts
Has a new target, needs to be mounted. 
Redoing simulation code

	Mooring failure
	Hardware is in. All tested except for galvanized. 

	Upside down sediment trap
	Waiting for new cups. Couplers are in and tight so union doesn’t come unscrewed and nipple stays in place.

	Larvae pump
	Rich has a functional enough motor that Rich can talk to. It’s ours, not DJ’s. He has a copy of composer. From the stack. 
Have final stack be wired by the time Rich gets back.
Seems to be working! Driver can spin the motor. Now split the max revolution velocity once it’s tuned up.
Dale can do tuning and config when he gets back. 
Johnny to cut more screen. 8 63 8 100
Is there a test cable for maxon?
Johnny has the index motor.
There is a hall sensor. Needs to take it to pot. 
Index motor comp- Dale has a plan for relieving the board
Aug 21st. Kim R has a method for cutting screens
Working on cables for pump

	Freeze dryer
	Ordered spare parts

	Wave glider
	Getting ready for Canon.

	Macro system
(aka shrimpoteuthis)
	Don’t ask till after cruise
Sidelined until the other aspects are done. Keep up momemtum and finish after cruise.
50 mm lens, higher contrast. Cut housing in half
Will we have a pointer laser ready?
Lid’s coming in the mail.
Johnny working on endcap. 
Test in dark
In 2020 Change to easier to use menu? Engineering logging?
To measure angle off horizontal- ~30 degrees. Move to 45. Mount battery at mud level. 
No purge port, use alkalines for lasers
Pressure test? Pump helium in to test weld?

	Cruise prep
	Alana to help pack palletainers
Johnny has built anchors for moorings. 
Add beacons to rescue float pack. Strobes and VHF. 
Francois is evaluating the elevator engineering.
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	Solo camera height, angles
	Not coming back. New mooring line will go on Solo camera and two inverted traps. 

	Rover
	Changing transducer. It’s bigger. Johnny to get it from Rover lab when he has time.

	30 year volume
	Ten papers submitted: 1 accepted fully. 5 in revision. 

	Olmo
	Revising draft

	Personnel schedules
	Rich-Sept 19-4 Oct
Alana- 9-17 October
Crissy 9 October



