	November 3, 2021 

	Lasers
	Need correction for distortion. Center of distortion is not the center of the image. Assymetrical barrel distortion. Sending pics to dan davis
Not doing lasers next Monday
Dan has been working on data from last calibration in June- got some promising results. Measure plastic animals

	Loop and Cross
	Very interested and thinks it’s publishable research. But he can’t promise we’d have something by July. Paul was able to fix some code issues to improve location data
Kent’s reporting to Paul today
Put Rich in the loop
Kent has been working a lot on that
Chris is helping him try to run some code on the wave glider 
Kent is testing his code on SES- Phase 2 ask for 80 hours of Kent’s time. Made a lot of progress and wants to finish it. Wait until we have targets out there

	Squirty 
	Need to put it on

	Macro system

	Testing worked.
On standby until next carson deployment

	Snappy
	Make more snappy boards
Expect a PO
Not till macro is working
Making more snappies
Alana to make setup- call in Rich to finish the working product
Alana to check notes
Need to work out bugs of new snappy. 
Don’t ask

	Rover export: PMEL, NOC
	Sent diagram
New contact of someone who can make the spheres
Chafey spheres

	SES prep
	Figure out fluid issue. 
Pulled small camera off, looks similar.
Ken: Get rid of o-ring lube and leaft the rest the same.
Plastic PVC was always turning white.
Can install batteries in a few hours. 
Discussing whether solution needs to be 50:50 DI ethanol. Going to replace tubes

	Rover troubleshooting
	Port rack controller is open and ready to test (Rich, Alana, Paul will do when they have time)
Need to open starboard rack
Don’t know why propulsion motor wasn’t running.
Did donuts for a few times, but then motor controller totally failed. 
Need to change lithium battery that powers the wake up
No water in motor controller
If doesn’t move, still take photos. Still did incubations.
During mission, some components stop trying once something goes bad. Add a “keep trying” aspect to the code. Log error and keep going. Once it found there was a failure in the communication it wen’t on the no-go list.
That one motor (stbd controller) isn’t returning status. On RS45 tied together. Can talk to one but not the other. Means comm line at least to one is good.
LF modem just get rid of it. Send to Benthos and say See!           This is no good!
MF modem battery is dead. 3 v left.

	Rover, SES comms
	Bring MF dunker, make sure davit works

	Benthos modem
	Don’t have MF yet. To be shipped 19 Nov
LF not yet mounted

	pH sensor
	On Solo frame

	Papers
	Rover paper in press- COVER SHOT!!
Larissa’s ms paper
Oxygen 
Yearly-hourly- compare community structre behavior to ecological variables- Later

	Eye-Ris camera
	Talking about taking it out today. On AUV. Check out Brett’s photo

	Cruise
	Waiting to find out about early 2022. January is best bet, depends on GOC

	ITS
	Ken to get an email from Monique

	Rich
	[bookmark: _GoBack]Is a grandpa!

	Personnel schedules
	Rich- out the last couple of weeks of the year
Crissy- Mid Dec 
Ken- some time




