DM6952HR
Power Relay dataModule®
16-Channel Mechanical Relay Output Module
for Industrial Applications

Operating Temperature -40° to +85°C


	[image: image1.jpg]




	DM6952HR-H Power Relay dataModule®

	



	Rugged IDAN™ Configuration


Features: 

· Outputs 

· 16 power relays with Form C contacts 

· 60 VA switching capacity 

· Switching current 

· 2 A at 30 VDC 

· 0.5 A at 125 VAC 

· 0.25 A at 220 VAC 

· Max switching voltage 220 VDC / VAC 

· Operate and release time 4 milliseconds 

· 1000 Vrms isolation 

· Expected life 

· Mechanical (at 180 cpm) 100,000,000 operations 

· Electrical at 2 A, 30 VDC resistive 500,000 operations 

· Connectors 

· -H: Standard 50 position 0.1" DIL headers 

· -S: Screw terminal blocks 

Description: 

The DM6952HR dataModule® combines on one board 16 power relay outputs. These relays may be used to reliably switch voltages from 5V DC to mains voltages of 220VAC. The onboard relays have two identical pairs of contacts. These contacts are connected on parallel. Both Normally Open (NO) and Normally Closed (NC) contacts are available on the I/O connectors. Use this board in applications such as AC or DC power circuit breaking, motor and actuator control or voltage level shifting. 

Software: 

· DOS  examples with source code. 

· Windows drivers with Visual C++ examples, source code, and API documentation. 

· Linux driver and examples with full source code and API documentation[image: image3.jpg]


 

Physical Attributes: 

· Dimensions: 90.17 mm L x 95.89 mm W (3.550 in L x 3.775 in W) 

· Weight: Approximately 0.15 Kg (0.34 lbs.) 

· Operating Temperature: -40° to +85°C: 90% humidity non-condensing 

· Storage Temperature: -55° to +125 °C 

· Power requirements:   1.25W (all relays active) @ 5 VDC typical 

Recommended Accessories:
· XT50: 3 foot, 50-pin, twisted-pair cable 

· TB50: 50-pin screw terminal board 

· XB50: 50-pin screw terminal board with prototyping area 

Documentation and Software Downloads:
· Hardware Manual 

· Drivers and Example Programs 

· Software Manual(s) 

Ordering Information
	Part Number
	Description
	OEM Price

	DM6952HR-H
	16 Relay Output dataModule®
 with headers
	$ 225

	DM6952HR-S
	16 Relay Output dataModule®
 with screw terminal blocks
	$ 245


