Load Test Report
Monday, February 09, 2009
	Company: MBARI

	Location: Moss Landing, CA


	Test Equipment: Allied Crane TK22-25, Load Cell, Dynamometer

	Structure: ALLIED CRANE TK22-25


	Load cell number:
	 :



	RATED LOAD: Retracted
	Pounds: 23,780


	RATED LOAD: Extended
	Pounds: 12,000


	TEST LOAD: Retracted
	Pounds: 21,450

	Dwell time: at 18,000 lbs
	Minutes: 15


Crane Assembly
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X = 11.75 inches
Y = 29 inches

Description:

The Load test was conducted onboard the Western Flyer dockside. The crane was lowered and rigged back to itself with the Docking Head installed. A load cell was placed between the crane base and the docking head to record the load. The load was raised to 21,450 lbs and then reduced to 18,100 lbs and held for 15 minutes.
Test rigging setup
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Test Results: PASSED
	Deflection:
	NONE


Prepared by: M.Brown: Monday, February 09, 2009
