Vicor Micro Carrier Board

Configuration Sheet

16 May 2008

Paul McGill

Application:       MARS Extension Cable SIIM for MOBB, distal end, experiment power  
Board Serial Number:     4                                      
Date:     16May08                                                   
Configuration Revision Number:     1.0.1              
Engineer:     Paul McGill                                       
Input Voltage:    375 V     
Output Voltage:     28 V     

Vicor Part Number:      V375C28C150BF              
Fuse Rating (F1)
Voltage:   500 V 
Current:  3.15 A    


Fast Blow         
Slow Blow    X   
Trim Up Resistor (R2)
No    X   
Yes        
Value:             
Trim Down Resistor (R4)
No    X   
Yes        
Value:             
Install Neon Flasher (NEON1, C3, R1, R5, R6, R7)


No         
Yes    X   
Install Vicor Shutdown Optoisolator (ISO1, J2)


No    X   
Yes          
