Vicor Micro Carrier Board

Configuration Sheet

16 May 2008

Paul McGill

Application:       MARS Extension Cable SIIM for MOBB, proximal end                           
Board Serial Number:     2                                      
Date:     16May08                                                   
Configuration Revision Number:     1.0.1              
Engineer:     Paul McGill                                       
Input Voltage:    48 V      
Output Voltage:     5 V      

Vicor Part Number:      V48C5H100BF                
Fuse Rating (F1)
Voltage:   250 V 
Current:    1 A     


Fast Blow         
Slow Blow    X   
Trim Up Resistor (R2)
No    X   
Yes        
Value:             
Trim Down Resistor (R4)
No    X   
Yes        
Value:             
Install Neon Flasher (NEON1, C3, R1, R5, R6, R7)


No    X   
Yes        
Install Vicor Shutdown Optoisolator (ISO1, J2)


No    X   
Yes        
