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Deployment Plan for CANON 31
Objectives

· CANON reconnaissance

· Power Management Performance Measurements

· Control Surface Duty Cycle Testing

	Budget is listed in A-hrs to reflect what vehicle will report while deployed.  Budgeted discharge rates are based on 15 volt battery bus.  This is conservative to ensure we have power at the end of the deployment. 

	
	
	Budget
	Actual

	Date / Day
	Activity / Mission
	Rate in Amps
	Duration in hours
	Cost in A-hrs
	Running Balance
	

	04/21, Thu
	
	
	
	
	250.0
	

	
	Reboot at pier, Restart at launch
	1.60
	0.50
	0.80
	249.2
	

	
	Transit to 3KM at 0.75 m/s
	0.75
	0.60
	0.45
	248.8
	

	
	Compass calibration
	1.60
	1.00
	1.60
	247.2
	

	
	triangle_control_elevator.xml ~ 180min run time
	1.60
	3.00
	4.80
	242.4
	

	
	Restart for fresh logs
	
	
	
	242.4
	

	
	YoYo transect to M0
	1.90
	2.57
	4.88
	237.5
	

	
	Run FrontFinder
	1.90
	10.00
	19.00
	218.5
	

	
	Low Energy Drift
	0.50
	14.00
	7.00
	211.5
	

	04/22, Fri
	
	
	
	
	211.5
	

	
	Low Energy Drift
	0.50
	24.00
	12.00
	199.5
	

	04/23, Sat
	
	
	
	
	199.5
	

	
	Run FrontFinder
	1.90
	10.00
	19.00
	180.5
	

	
	Low Energy Drift
	0.50
	14.00
	7.00
	173.5
	

	04/24, Sun
	
	
	
	
	173.5
	

	
	Low Energy Drift
	0.50
	24.00
	12.00
	161.5
	

	04/25, Mon
	
	
	
	
	161.5
	

	
	Run FrontFinder
	1.50
	10.00
	15.00
	146.5
	

	
	Low Energy Drift
	0.50
	14.00
	7.00
	139.5
	

	04/26, Tue
	
	
	
	
	139.5
	

	
	Chlorophyll tracking mission
	1.90
	9.00
	17.10
	122.4
	

	
	Robot Dance through the night
	2.20
	15.00
	33.00
	89.4
	

	04/27, Wed
	
	
	
	
	89.4
	

	
	Robot Dance through the night
	2.20
	15.00
	33.00
	56.4
	

	
	Low Energy Drift
	0.50
	9.00
	4.50
	51.9
	

	04/28, Thu
	
	
	
	
	51.9
	

	
	Robot Dance through the night
	2.20
	15.00
	33.00
	18.9
	

	
	Low Energy Drift
	0.50
	9.00
	4.50
	14.4
	

	04/29, Fri
	
	
	
	
	14.4
	

	
	Transit to M0 to 3KM at .75 m/s
	0.75
	3.00
	2.25
	12.1
	

	
	Recovery Reserve
	
	
	10.00
	2.1
	


