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Vehicle Close Out Check List



1. Vehicle name

2. Date of last Pressure Vessel close out. . ___________
3. Forward Wet Volume 
a. Alternate Location Devices

i. Pinger RJE

1. Model ULB-350/37

2. Serial DT16485

3. Freq 37KHZ 1pps

4. New Batteries on ______________

ii. Transponder - Benthos

1. Model UAT-376(006199)

2. Serial 498

3. Rcv 26 KHz

4. TX 29 KHz

5. Pressure tested to 1000 psi 

6. New Batteries on __________________

b. Bow Bracket Assembly

i. Short

ii. Long – Turbulence

iii. Long – Docking

iv. Long – Other

c. External Instrument payload

	Sensor
	Serial number
	Calibration date
	Notes (number of matching external head)

	CT Sensor
	
	
	

	Flourometer
	
	
	

	DVL
	
	
	

	Compass
	
	
	

	PAR
	
	
	

	ISUS
	
	
	

	DO
	
	
	

	DAT
	
	
	

	Turbulence
	
	
	

	  other
	
	
	


d. Install Forward Fairing

e. Flourometer adjusted flush with skin

f. PAR adjusted flush with skin

4. Aft Wet Volume

a. Alternate Location Device - ARGOS

i. Model __________________

ii. Serial number __________________

iii. Configuration file saved to deployment folder__________________

iv. Number of transmission used__________________

b. CS Actuators

i. 0 degree at mid range of travel

ii. Oil comp full

c. Drop Weight installed

d. Aft fairing is partially installed on vehicle

e. Antenna connectors installed and tight
i. Iridium

ii. GPS

iii. Freewave

5. Ready for Deployment Checklist

6. External Instrument payload
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