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Vehicle Close Out Check List



1. Vehicle name Tethys
2. Date of last Pressure Vessel close out. . ___________
3. Forward Wet Volume 
a. Acoustic Location Device
i. Transponder - Benthos

1. Model UAT-376(006199)

2. Serial 498

3. Rcv 26 KHz

4. TX 29 KHz

5. Pressure tested to 1000 psi 

6. Battery Voltage ___9.15VDC_ on _5/28/2013__

b. Bow Bracket Assembly 
i. Short / Long – Turbulence / Long – Docking / Long – Other

ii. Short nose with modified CT clamshell.

c. External Instrument payload

	Sensor
	Installed?
	Serial number
	Calibration date
	Notes (number of matching external head)

	CT Sensor
	Y
	
	
	

	Flourometer
	Y
	
	
	

	DVL
	Y
	
	
	

	Compass
	Y
	
	
	

	PAR
	Y
	
	
	

	ISUS
	Y
	
	
	

	DO
	Y
	
	
	

	DAT
	N
	
	
	

	Turbulence
	N
	
	
	

	  other
	N
	
	
	


d. Install Forward Fairing

e. Flourometer adjusted flush with skin

f. PAR adjusted flush with skin

4. Aft Wet Volume

a. Alternate Location Device - ARGOS

i. Model __________________

ii. Serial number __________________

iii. Configuration file saved to deployment folder__________________

iv. Number of transmission used__________________

b. CS Actuators

i. 0 degree at mid range of travel

ii. Oil comp full

c. Drop Weight installed

d. Aft fairing is partially installed on vehicle

e. Antenna connectors installed and tight
i. Iridium

ii. GPS

iii. Freewave

5. Ready for Deployment Checklist

6. External Instrument payload

Four pounds of lead aft.
Five pounds of lead forward
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